Initial DDRB: 0x00

Initial PORTB: 0x00

Port B is all outputs set to 0.

Stack Pointer: 0x10FF

R00: 0xFF

The Program looped 4 times.

To change the number of loops, change: ldi I, $04

R01: 0xAA

R02: 0x0F

R03: 0x0F

**PART 2:**

Stack Pointer: 0x10FD

FUNCTION: ba0e